Annexure-I

COST BREAK UP FOR PACK HOUSE
	Requirements and Costing for Pack House

	Sl. No
	Detail of structure
	Specifications/Details
	Qty
	Units
	Unit rate (Rs)
	Total Cost (Rs)

	A
	Land
	Near Metal road, near well, power pole etc
	500
	Yds
	Farmer's Own
	A

	B
	Expenditure Item
	
	
	
	
	

	1
	Civil Structure
	
	
	
	
	

	1.1
	Site leveling etc
	Leveling land and to make it motorable inside the premises
	500
	Yds
	
	400000

	1.2
	30X20' (9x6 Mts) Packing hall
	30X20 ft with GI/Asbestos roof, Hard cement flooring, GI / Iron Windows, doors.
	600
	Sft
	
	

	2
	Mechanical
	
	
	
	
	

	2.1
	Packing /grading Table
	4'X8' of GI or SS material, with 100mm side protection to stop roll off and with provision to drain water
	1
	No’s
	14000
	14000

	2.2
	Movable Trolleys
	
	1
	No’s
	5000
	5000

	2.3
	Washing sheets (HDPE)
	Of plastic of not less than 5' length and 2.6' ft width
	1
	No’s
	3750
	3750

	2.4
	Electronic Weighing Machine
	To weigh up to 300 kgs with an accuracy of + or - 0.1 Kg with at least 400X 600mm plat form
	1
	No’s
	8000
	8000

	2.5
	Desaping Units (for Mango growers only)
	1.2 – 1.5mtr.(L)x0.8 – 1.0mtr.(W) x20cm (H);GI rods covered with ½”PVC Pipes
	2
	No’s
	1500
	3000

	2.6
	Dhapoli Harvesters (for Mango growers only)
	
	5
	No’s
	400
	2000

	3
	Electrical
	
	
	
	
	

	3.1
	Meter with connection
	Single Phase or three phase connection including deposit
	1
	No’s
	6500
	6500

	3.2
	Electrical Wiring with fuses, switches, holders, bulbs, fans etc.
	5 Tube lights, 3 Fans with 2 Hrs. back up
	1
	Set
	7000
	7000

	4
	Water tank with support
	Plastic “Sintex” or equivalent or cement based located at height either outside or with separate support of at least 2000 liters capacity
	1
	No’s
	12500
	12500

	5
	Other assets Small office table, three chairs, almairah, Wooden showels
	
	1
	LS
	5000
	5000

	6
	Plastic Crates
	40 Ltrs. Capacity (25 Kgs)
	60
	No’s
	280
	16800

	7
	Inverter (Optional)
	
	
	1
	
	

	
	
	
	
	
	TOTAL
	4,83,550


	
Pattern of Assistance: Unit Cost LIMITED TO Rs.4,80,000/- (Rupees Four Lakh eighty thousand only) and assistance admissible is 50%




	Annexure-II

	ESTIMATE FOR THE PROPOSED MODEL PACK HOUSE - SIZE - 30' X 20' = 600 SFTUNDER M.I.D.H.

	S.NO.
	Description of work
	Quantity
	Rate
	Per
	Amount (Rs)

	


1
	Earth work excavation in all types of soils for walls and for columns footings as per drawing or as directed by the including dewatering shoring, sheeting, shuttering if necessary all leads, lifts, delifts and back filling trenches with watering and tamping on either of stone masonry upto Ground level, spreading and levelling surplus earth as directed wih in the premises etc., complete
	


20.60
	


391.00
	


Cum.
	


8055

	

2
	Providing and laying in line and level in cement concrete (1:4:8) Proportion using 40mm guage hard granite well graded aggregate including dewatering, machine mixing, shuttering, vibrating, ramming curing, all leads, lifts, delifts, etc., complete.
	
	
	
	

	a)
	Under foundations
	2.26
	5000.00
	Cum.
	11300

	b)
	Under flooring
	4.29
	5000.00
	Cum.
	21450

	
3
	Providing and constructing CRS masonry with cement Mortar (1:6) Proportion in basement including curing, dewatering, lead, lift, delift etc., complete
	
17.18
	
3600.00
	
Cum.
	
61848

	
4
	Earth filling in basement and/or plinth with soils of approved quality/borrowed with standard specifications in layers of 150 mm to 230 mm (6" to 9") including watering and tamping and thoroughly consolidating.
	
15.15
	
270.00
	
Cum.
	
4090

	
5
	RCC WORK: Reinforced concrete work conforming to IS 456 in M20 Proportion using 6mm to 20mm guage metal with steel centring or form work required including mild or tor steel reinforcement.
	
1.03
	
9549.00
	
Cum.
	
9835

	

6
	Providing and constructing Super structure in 230mm (9") thick wall in cement mortar (1:6) in line and level including watering, curing, lead, lift, delift, cost and conveyance of all materials to site, all incidental and operational charges etc., complete
	

19.90
	

8000.00
	

Cum.
	

159200

	



7
	Providing and applying 20mm (3/4") thick cement plastering to walls in two coats out of which first coat of 16mm (5/8") thick shall be in ecment mortar (1:5) Proportion and the second coat of 4mm (1/8") thickness in cement mortar (1:3) Proportion with sponge finish or fine finish as directed, in line and level including watering, curing, all leads, lifts, delifts, cost and conveyance of all materials to site, all incidental and operational all charges etc., complete.
	



190.24
	



500.00
	




Sqm
	



90120




	
8
	Providing and applying raised and cut pointing over exposed surface of CRS masonry in cement mortar (1:1) including all cost of material, labour, lead, lift, etc., complete course.
	
18.58
	
210.00
	
Sqm
	
3902

	

9
	Providing and laying cement flooring in cement mortar (1:3) with a floating coat of cement slurry and making squares of 2'X2' including all operational charges curing, lead, lift, etc., complete.
	

49.00
	

1200.00
	

Sqm
	

58800

	



10
	Supply and fixing of flush doors in M.S. box frame in 125 X 64mm thick fabricated in 1mm thick sheet with shutter of black board solid core 35mm thick, covered both the surfaces with commercial ply, duly painted two coats of enamel with luppum putty, with the following specifications etc., including cost of c.c. bed blocks in (1:2:4) filling the inner portion of frame with cement mortar (1:8) etc.,completer
	












2.00
	












7160.00
	












Nos
	












14320

	a)
	M.S. box frame: 127mm X 64mm 12mm X 35mm rebate
	
	
	
	

	b)
	Hold Fasts: iron hold fasts, 6 Nosembeded in cement concrete (1:2:4)
	
	
	
	

	
c)
	Hinges: 150mm X 40mm iron anodized butt hinges with nettle fold screws 3 Nos or as required
	
	
	
	

	d)
	Shutter: 40mm thick black board of solid core of approved quality
	
	
	
	

	e)
	Tower Bolts: aluminium
	
	
	
	

	
	i) 200mm long - 1 No
	
	
	
	

	
	ii) 150mm long - 1 No
	
	
	
	

	f)
	Handle: aluminum
	
	
	
	

	
	i) 150mm long - 2 Nos
	
	
	
	

	g)
	Stoppers: double barrel
	
	
	
	

	h)
	Aldrop: - 1 No
	
	
	
	

	
i)
	Enamel painting two coats with wood primer and two coats of luppum finish of approved quality, colour and shade
	
	
	
	



	
11
	Supplying and fixing of Glazed M.S. Windows with 10mm square guard bars at 150mm c/c including hardware and 4mm glass
	
11.90
	
4000.00
	
Sqm
	
47600

	

12
	Supplying fabricating and erecting in position M.S. tubular trusses in 2" dia "B" class pipe including providing and applying two coats of enamel paint with anti corrosive red oxide primer including all operational charges lead, lift etc., complete
	

0.75
	

75000
	

M.T
	

56250

	
13
	Providing and laying asbestos sheets roof with charminar asbestos sheets with the required ridge piece including all operational charges lead, lift, etc., complete.
	
59.94
	
300.00
	
Sqm
	
17982

	
14
	Providing and applying two coats of suryacem paint over the plastered surfaces including cleaning the floor etc., complete.
	
183.45
	
40
	
Sqm
	
7338


	
	
	
	
	Rs
	572090/-




Pattern of Assistance: Unit Cost LIMITED TO Rs.4,80,000/- (Rupees Four Lakh eighty thousand only) and assistance admissible is 50%
	Note

	1
	Each Pack house should also be given crates under other schemes to use within pack house as a rule

	2
	Second packing, grading table is preferable

	3
	Inverter is preferable, as power cuts may prevail in villages

	4
	If any other scheme provides for Solar lights, they should be encouraged





Signature of Civil Engineer.
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of the Regd. Civil Engineer with Seal.

Signature




